1. calculate cost based on number of turbine
2. suitable place through wind speed from 8 m/s cut in to 17m/s cutout min&&max
3. forbid turbines to be installed too close to each other (at less than 3D distance)
4. at the same direction of wind distance between turbines from 5 to 9 wal3mode from 3 to 5
5. pdf paper e5tar AL median w3mal iteration wtla3 efficient solution ale hya 7 we 4